<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="163.81" y2="0" width="0" layer="20"/>
<wire x1="163.81" y1="0" x2="163.83" y2="86.36" width="0" layer="20"/>
<wire x1="163.83" y1="86.36" x2="0" y2="86.36" width="0" layer="20"/>
<wire x1="0" y1="86.36" x2="0" y2="0" width="0" layer="20"/>
<text>C1</text>
<text>10uF</text>
<text>C2</text>
<text>10uF</text>
<text>DS18B20</text>
<text>IC1</text>
<text>74LS595N</text>
<text>IC2</text>
<text>74LS595N</text>
<text>A15,2mm</text>
<text>IC3</text>
<text>IC6</text>
<text>IC_74141-DIP-16</text>
<text>IC7</text>
<text>IC_74141-DIP-16</text>
<text>IC8</text>
<text>IC_74141-DIP-16</text>
<text>IC9</text>
<text>IC_74141-DIP-16</text>
<text>IC10</text>
<text>IC_74141-DIP-16</text>
<text>IC11</text>
<text>IC_74141-DIP-16</text>
<text>IC12</text>
<text>74LS595N</text>
<text>J2</text>
<text>WARNING! HIGH VOLTAGE! 170V!</text>
<text>R1</text>
<text>R2</text>
<text>R3</text>
<text>R4</text>
<text>R5</text>
<text>R6</text>
<text>R7</text>
<text>R8</text>
<text>R9</text>
<text>RTC</text>
<text>S1</text>
<text>S2</text>
<text>S3</text>
<text>TUBE-1</text>
<text>TUBE-2</text>
<text>TUBE-3</text>
<text>TUBE-4</text>
<text>TUBE-5</text>
<text>TUBE-6</text>
<text>ARDUINO_MINI</text>
<text>NIXIE-BOT
</text>
<text>SCOTT-BOT.com</text>
<text>12V</text>
<text>5V</text>
<text>GND</text>
<text>Mr. Gecko</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="78XXL">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="DIL16">
<description>DIL-16</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-10UF-25V">
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="ScottCustom">
<packages>
<package name="ARDUINO_MINI">
</package>
<package name="DS18B20">
</package>
<package name="NIXIE_PWR_SUPPLY">
</package>
<package name="SCOTT_RTC">
</package>
<package name="IN-14">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
<package name="SWITCH-SPDT">
</package>
</packages>
</library>
<library name="con-jack">
<description>&lt;b&gt;Jacks&lt;/b&gt;&lt;p&gt;
Power Connectors&lt;br&gt;
Phone Connectors&lt;br&gt;
Cinch Connectors&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SPC4077">
<description>&lt;b&gt;DC POWER JACK 2mm&lt;/b&gt;&lt;br&gt; Right Angle, Through Hole, Rated 5A at 16VDC, PC Terminals&lt;p&gt;
Source: www.spctechnology.com .. 84N1161.pdf&lt;br&gt;
Distributor: &lt;b&gt;Farnell (www.Farnell.de)&lt;/b&gt;&lt;br&gt;
Created by Robert Siegler</description>
</package>
</packages>
</library>
<library name="holes">
<description>&lt;b&gt;Mounting Holes and Pads&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="3,6-PAD">
<description>&lt;b&gt;MOUNTING PAD&lt;/b&gt; 3.6 mm, round</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA03-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R2" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R3" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R5" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R6" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="R7" library="SparkFun" package="AXIAL-0.4" value=""/>
<element name="IC6" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC7" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC8" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC9" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC10" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC11" library="dp_devices" package="DIL16" value="IC_74141-DIP-16"/>
<element name="IC12" library="SparkFun" package="DIL16" value="74LS595N"/>
<element name="IC1" library="SparkFun" package="DIL16" value="74LS595N"/>
<element name="IC2" library="SparkFun" package="DIL16" value="74LS595N"/>
<element name="IC3" library="SparkFun" package="78XXL" value=""/>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="C2" library="SparkFun-Passives" package="CPOL-RADIAL-10UF-25V" value="10uF"/>
<element name="U$10" library="ScottCustom" package="ARDUINO_MINI" value="ARDUINO_MINI"/>
<element name="DS18B20" library="ScottCustom" package="DS18B20" value=""/>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="NIXIE_PWR_SUPPLY" library="ScottCustom" package="NIXIE_PWR_SUPPLY" value=""/>
<element name="S1" library="SparkFun-Electromechanical" package="TACTILE-PTH" value=""/>
<element name="R8" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-PTH" value=""/>
<element name="R9" library="SparkFun-Passives" package="AXIAL-0.4" value=""/>
<element name="J2" library="con-jack" package="SPC4077" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="RTC" library="ScottCustom" package="SCOTT_RTC" value=""/>
<element name="S3" library="SparkFun-Electromechanical" package="SWITCH-SPDT" value=""/>
<element name="TUBE-1" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="TUBE-2" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="TUBE-3" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="TUBE-4" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="TUBE-5" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="TUBE-6" library="ScottCustom" package="IN-14" value="IN-14"/>
<element name="H1" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="H2" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="H3" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="H4" library="holes" package="3,6-PAD" value="MOUNT-PAD-ROUND3.6"/>
<element name="PWR" library="con-lstb" package="MA03-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC6" pad="12"/>
<contactref element="IC9" pad="12"/>
<contactref element="IC10" pad="12"/>
<contactref element="IC7" pad="12"/>
<contactref element="IC8" pad="12"/>
<contactref element="IC11" pad="12"/>
<contactref element="IC12" pad="8"/>
<contactref element="IC12" pad="13"/>
<contactref element="U$10" pad="23"/>
<contactref element="U$10" pad="4"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC2" pad="13"/>
<contactref element="IC3" pad="GND"/>
<contactref element="DS18B20" pad="1"/>
<contactref element="NIXIE_PWR_SUPPLY" pad="GND"/>
<contactref element="NIXIE_PWR_SUPPLY" pad="GND2"/>
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="8"/>
<contactref element="R8" pad="P$1"/>
<contactref element="R9" pad="P$1"/>
<contactref element="RTC" pad="4"/>
<contactref element="J2" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="PWR" pad="3"/>
</signal>
<signal name="5V">
<contactref element="IC6" pad="5"/>
<contactref element="IC7" pad="5"/>
<contactref element="IC8" pad="5"/>
<contactref element="IC11" pad="5"/>
<contactref element="IC10" pad="5"/>
<contactref element="IC9" pad="5"/>
<contactref element="IC12" pad="16"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC12" pad="10"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC3" pad="OUT"/>
<contactref element="C2" pad="1"/>
<contactref element="DS18B20" pad="3"/>
<contactref element="R4" pad="P$2"/>
<contactref element="S1" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="RTC" pad="5"/>
<contactref element="S3" pad="1"/>
<contactref element="S1" pad="4"/>
<contactref element="S2" pad="4"/>
<contactref element="PWR" pad="2"/>
</signal>
<signal name="V+">
<contactref element="R1" pad="P$2"/>
<contactref element="R7" pad="P$2"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
<contactref element="R2" pad="P$2"/>
<contactref element="NIXIE_PWR_SUPPLY" pad="HV+"/>
</signal>
<signal name="N$8">
<contactref element="IC9" pad="15"/>
<contactref element="TUBE-1" pad="2"/>
</signal>
<signal name="N$67">
<contactref element="IC7" pad="6"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$68">
<contactref element="IC7" pad="7"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$69">
<contactref element="IC7" pad="4"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$70">
<contactref element="IC7" pad="3"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$71">
<contactref element="IC9" pad="6"/>
<contactref element="IC12" pad="1"/>
</signal>
<signal name="N$72">
<contactref element="IC9" pad="7"/>
<contactref element="IC12" pad="2"/>
</signal>
<signal name="N$73">
<contactref element="IC9" pad="4"/>
<contactref element="IC12" pad="3"/>
</signal>
<signal name="N$74">
<contactref element="IC9" pad="3"/>
<contactref element="IC12" pad="15"/>
</signal>
<signal name="N$75">
<contactref element="IC11" pad="6"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$76">
<contactref element="IC11" pad="7"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$77">
<contactref element="IC11" pad="4"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$78">
<contactref element="IC11" pad="3"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="N$79">
<contactref element="IC6" pad="3"/>
<contactref element="IC12" pad="4"/>
</signal>
<signal name="N$80">
<contactref element="IC12" pad="5"/>
<contactref element="IC6" pad="6"/>
</signal>
<signal name="N$81">
<contactref element="IC6" pad="7"/>
<contactref element="IC12" pad="6"/>
</signal>
<signal name="N$82">
<contactref element="IC12" pad="7"/>
<contactref element="IC6" pad="4"/>
</signal>
<signal name="N$83">
<contactref element="IC12" pad="9"/>
<contactref element="IC1" pad="14"/>
</signal>
<signal name="N$84">
<contactref element="IC1" pad="9"/>
<contactref element="IC2" pad="14"/>
</signal>
<signal name="N$85">
<contactref element="IC10" pad="3"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="N$86">
<contactref element="IC10" pad="6"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$87">
<contactref element="IC10" pad="7"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$88">
<contactref element="IC10" pad="4"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$90">
<contactref element="IC8" pad="3"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="N$91">
<contactref element="IC8" pad="6"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$92">
<contactref element="IC8" pad="7"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="N$93">
<contactref element="IC8" pad="4"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$89">
<contactref element="IC12" pad="14"/>
<contactref element="U$10" pad="8"/>
</signal>
<signal name="N$94">
<contactref element="IC12" pad="11"/>
<contactref element="IC1" pad="11"/>
<contactref element="IC2" pad="11"/>
<contactref element="U$10" pad="10"/>
</signal>
<signal name="N$95">
<contactref element="IC12" pad="12"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="12"/>
<contactref element="U$10" pad="9"/>
</signal>
<signal name="N$97">
<contactref element="DS18B20" pad="2"/>
<contactref element="U$10" pad="5"/>
<contactref element="R4" pad="P$1"/>
</signal>
<signal name="VIN">
<contactref element="IC3" pad="IN"/>
<contactref element="C1" pad="1"/>
<contactref element="NIXIE_PWR_SUPPLY" pad="V+"/>
<contactref element="J2" pad="3"/>
<contactref element="PWR" pad="1"/>
</signal>
<signal name="N$96">
<contactref element="S2" pad="1"/>
<contactref element="S2" pad="2"/>
<contactref element="R9" pad="P$2"/>
<contactref element="U$10" pad="13"/>
</signal>
<signal name="N$101">
<contactref element="S1" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="R8" pad="P$2"/>
<contactref element="U$10" pad="14"/>
</signal>
<signal name="N$98">
<contactref element="U$10" pad="A5"/>
<contactref element="RTC" pad="2"/>
</signal>
<signal name="N$99">
<contactref element="U$10" pad="A4"/>
<contactref element="RTC" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="IC9" pad="8"/>
<contactref element="TUBE-1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="IC9" pad="9"/>
<contactref element="TUBE-1" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="IC9" pad="13"/>
<contactref element="TUBE-1" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="IC9" pad="14"/>
<contactref element="TUBE-1" pad="6"/>
</signal>
<signal name="N$13">
<contactref element="IC9" pad="11"/>
<contactref element="TUBE-1" pad="7"/>
</signal>
<signal name="N$14">
<contactref element="IC9" pad="10"/>
<contactref element="TUBE-1" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="IC9" pad="1"/>
<contactref element="TUBE-1" pad="9"/>
</signal>
<signal name="N$16">
<contactref element="IC9" pad="2"/>
<contactref element="TUBE-1" pad="0"/>
</signal>
<signal name="N$17">
<contactref element="IC6" pad="16"/>
<contactref element="TUBE-2" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="IC6" pad="15"/>
<contactref element="TUBE-2" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="IC6" pad="8"/>
<contactref element="TUBE-2" pad="3"/>
</signal>
<signal name="N$20">
<contactref element="IC6" pad="9"/>
<contactref element="TUBE-2" pad="4"/>
</signal>
<signal name="N$21">
<contactref element="IC6" pad="13"/>
<contactref element="TUBE-2" pad="5"/>
</signal>
<signal name="N$22">
<contactref element="IC6" pad="14"/>
<contactref element="TUBE-2" pad="6"/>
</signal>
<signal name="N$23">
<contactref element="IC6" pad="11"/>
<contactref element="TUBE-2" pad="7"/>
</signal>
<signal name="N$24">
<contactref element="IC6" pad="10"/>
<contactref element="TUBE-2" pad="8"/>
</signal>
<signal name="N$25">
<contactref element="IC6" pad="1"/>
<contactref element="TUBE-2" pad="9"/>
</signal>
<signal name="N$26">
<contactref element="IC6" pad="2"/>
<contactref element="TUBE-2" pad="0"/>
</signal>
<signal name="N$27">
<contactref element="IC7" pad="16"/>
<contactref element="TUBE-3" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="IC7" pad="15"/>
<contactref element="TUBE-3" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="IC7" pad="8"/>
<contactref element="TUBE-3" pad="3"/>
</signal>
<signal name="N$30">
<contactref element="IC7" pad="9"/>
<contactref element="TUBE-3" pad="4"/>
</signal>
<signal name="N$31">
<contactref element="IC7" pad="13"/>
<contactref element="TUBE-3" pad="5"/>
</signal>
<signal name="N$32">
<contactref element="IC7" pad="14"/>
<contactref element="TUBE-3" pad="6"/>
</signal>
<signal name="N$33">
<contactref element="IC7" pad="11"/>
<contactref element="TUBE-3" pad="7"/>
</signal>
<signal name="N$34">
<contactref element="IC7" pad="10"/>
<contactref element="TUBE-3" pad="8"/>
</signal>
<signal name="N$35">
<contactref element="IC7" pad="1"/>
<contactref element="TUBE-3" pad="9"/>
</signal>
<signal name="N$36">
<contactref element="IC7" pad="2"/>
<contactref element="TUBE-3" pad="0"/>
</signal>
<signal name="N$37">
<contactref element="IC10" pad="16"/>
<contactref element="TUBE-4" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="IC10" pad="15"/>
<contactref element="TUBE-4" pad="2"/>
</signal>
<signal name="N$39">
<contactref element="IC10" pad="8"/>
<contactref element="TUBE-4" pad="3"/>
</signal>
<signal name="N$40">
<contactref element="IC10" pad="9"/>
<contactref element="TUBE-4" pad="4"/>
</signal>
<signal name="N$41">
<contactref element="IC10" pad="13"/>
<contactref element="TUBE-4" pad="5"/>
</signal>
<signal name="N$42">
<contactref element="IC10" pad="14"/>
<contactref element="TUBE-4" pad="6"/>
</signal>
<signal name="N$43">
<contactref element="IC10" pad="11"/>
<contactref element="TUBE-4" pad="7"/>
</signal>
<signal name="N$44">
<contactref element="IC10" pad="10"/>
<contactref element="TUBE-4" pad="8"/>
</signal>
<signal name="N$45">
<contactref element="IC10" pad="1"/>
<contactref element="TUBE-4" pad="9"/>
</signal>
<signal name="N$46">
<contactref element="IC10" pad="2"/>
<contactref element="TUBE-4" pad="0"/>
</signal>
<signal name="N$47">
<contactref element="IC11" pad="16"/>
<contactref element="TUBE-5" pad="1"/>
</signal>
<signal name="N$48">
<contactref element="IC11" pad="15"/>
<contactref element="TUBE-5" pad="2"/>
</signal>
<signal name="N$49">
<contactref element="IC11" pad="8"/>
<contactref element="TUBE-5" pad="3"/>
</signal>
<signal name="N$50">
<contactref element="IC11" pad="9"/>
<contactref element="TUBE-5" pad="4"/>
</signal>
<signal name="N$51">
<contactref element="IC11" pad="13"/>
<contactref element="TUBE-5" pad="5"/>
</signal>
<signal name="N$52">
<contactref element="IC11" pad="14"/>
<contactref element="TUBE-5" pad="6"/>
</signal>
<signal name="N$53">
<contactref element="IC11" pad="11"/>
<contactref element="TUBE-5" pad="7"/>
</signal>
<signal name="N$54">
<contactref element="IC11" pad="10"/>
<contactref element="TUBE-5" pad="8"/>
</signal>
<signal name="N$55">
<contactref element="IC11" pad="1"/>
<contactref element="TUBE-5" pad="9"/>
</signal>
<signal name="N$56">
<contactref element="IC11" pad="2"/>
<contactref element="TUBE-5" pad="0"/>
</signal>
<signal name="N$57">
<contactref element="IC8" pad="16"/>
<contactref element="TUBE-6" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="IC8" pad="15"/>
<contactref element="TUBE-6" pad="2"/>
</signal>
<signal name="N$59">
<contactref element="IC8" pad="8"/>
<contactref element="TUBE-6" pad="3"/>
</signal>
<signal name="N$60">
<contactref element="IC8" pad="9"/>
<contactref element="TUBE-6" pad="4"/>
</signal>
<signal name="N$61">
<contactref element="IC8" pad="13"/>
<contactref element="TUBE-6" pad="5"/>
</signal>
<signal name="N$62">
<contactref element="IC8" pad="14"/>
<contactref element="TUBE-6" pad="6"/>
</signal>
<signal name="N$63">
<contactref element="IC8" pad="11"/>
<contactref element="TUBE-6" pad="7"/>
</signal>
<signal name="N$64">
<contactref element="IC8" pad="10"/>
<contactref element="TUBE-6" pad="8"/>
</signal>
<signal name="N$65">
<contactref element="IC8" pad="1"/>
<contactref element="TUBE-6" pad="9"/>
</signal>
<signal name="N$66">
<contactref element="IC8" pad="2"/>
<contactref element="TUBE-6" pad="0"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="P$1"/>
<contactref element="TUBE-1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="R7" pad="P$1"/>
<contactref element="TUBE-2" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="R3" pad="P$1"/>
<contactref element="TUBE-3" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="P$1"/>
<contactref element="TUBE-4" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="R6" pad="P$1"/>
<contactref element="TUBE-5" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R5" pad="P$1"/>
<contactref element="TUBE-6" pad="A"/>
</signal>
<signal name="N$100">
<contactref element="U$10" pad="21"/>
<contactref element="S3" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="TUBE-1" pad="1"/>
<contactref element="IC9" pad="16"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
